Task table

Task table is for the cpu so it can load values into the registers and its permisions so the proccess can contiune. Each block is a word

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| R00 | R01 | R02 | R03 | R04 | R05 | R06 | R07 |
| R08 | R09 | R10 | R11 | R12 | R13 | R14 | R15 |
| R16 | R17 | R18 | R19 | R20 | R21 | R22 | R23 |
| R24 | R25 | R26 | R27 | R28 | R29 | R30 | R31 |
| Permissions | Flags |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |